|  |  |  |
| --- | --- | --- |
|   |        |   |
|  | **Name of the company:** | **Operating Instructions** | **Date:** |   |
|   |   |
|   |   |
|   | **Working area:****Clamp silage** | **Activity: Filling, driving, removal** | **Signature:** |   |
|   |   |
|   |   |
|   | **DESIGNATION** |   |
|   | **Clamp silages** |   |
|   |   |
|   |   |
|   | **DANGERS TO HUMANS AND THE ENVIRNOMENT** |   |
|   | W001 Allgemeines Warnzeichen (Dieses Zeichen darf nur in Verbindung mit einem Zusatzzeichen angewendet werden, das die Gefahr konkretisiert) | * Danger from vehicle traffic, vehicle crash.
* Slipping and missing a step when getting on and off vehicles.
* Slipping, stumbling and falling on the silo cover or the slippery silo floor.
* Danger from falling silage masses at the removal point.
* Falling from the cutting edge or the silo wall.x
 | F:\svlfg\400_Praevention\401_GuQ\02_Allgemein\70_Medien\15_Symbole\ASR A1.3\Warnzeichen\GIF\w008.gif |   |
|   | **PROTECTIVE MEASURES AND RULES OF CONDUCT** |   |
|   | F:\svlfg\400_Praevention\401_GuQ\02_Allgemein\70_Medien\15_Symbole\ASR A1.3\Gebotszeichen\m008.gifF:\svlfg\400_Praevention\401_GuQ\02_Allgemein\70_Medien\15_Symbole\ASR A1.3\Gebotszeichen\m018.gif | x* Prevent unauthorised individuals (onlookers) from entering the silo.
* Employees and other involved parties (e.g. service providers) should receive instruction.
* Wear safety shoes/boots (S3/S5).
* Clean ascents of vehicles for silage or substrate removal regularly!
* Do not jump on to or down from vehicles, e.g. for silage or substrate removal. Climb off backwards
* Only use appropriate removal technology with a driver protection roof.
* Avoid undercuts at the removal location or eliminate them immediately.
* When uncovering the silo foil, a minimum distance of 2 metres from the cutting edge must be maintained. If necessary, suitable aids should be used to retract the film or remove the sandbags/tyres, or mobile railings or rope protection with suitable attachment points are used.
* Mobile silo walls are secured against persons falling inwards and outwards, e.g. by railings or an embankment (vertical distance between the embankment and top edge of the wall 1 m).
* Check protective devices for stability and functionality.x
 | F:\svlfg\400_Praevention\401_GuQ\02_Allgemein\70_Medien\15_Symbole\ASR A1.3\Verbotszeichen\GIF\d-p006.gif |   |
|   | **WHAT TO DO IN THE CASE OF MALFUNCTIONS** |   |
|   |  | * Immediately cordon off the danger areas!
 |  |   |
|   | **WHAT TO DO IN THE CASE OF ACCIDENTS – FIRST-AID – EMERGENCY TEL. NO. 112** |   |
|   | E004 Notruftelefon | * Carry out emergency measures at the scene of the accident!
* Call the emergency services/an emergency doctor!

First aider:………………………………………………………………………………………... | E003 Erste Hilfe |   |
|   | **Maintenance**  |   |
|   |  | * Replace or repair missing or damaged fall protection devices immediately!
 |  |   |
|  | **CONSEQUENCES OF NON-COMPLIANCE** |  |
|  |  | * Health consequences: Possibility of very serious or fatal injuries!x
 | www.svlfg.de |  |
|   |       |  |