|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  | | | | |  |
|  | **Name of the company:** | | **Operating Instructions** | **Date:** | |  |
|  |  |
|  |  |
|  | **Working area:**  **Clamp silage** | | **Activity: Filling, driving, removal** | **Signature:** | |  |
|  |  |
|  |  |
|  | **DESIGNATION** | | | | |  |
|  | **Clamp silages** | | | | |  |
|  |  |
|  |  |
|  | **DANGERS TO HUMANS AND THE ENVIRNOMENT** | | | | |  |
|  | W001 Allgemeines Warnzeichen (Dieses Zeichen darf nur in Verbindung mit einem Zusatzzeichen angewendet werden, das die Gefahr konkretisiert) | * Danger from vehicle traffic, vehicle crash. * Slipping and missing a step when getting on and off vehicles. * Slipping, stumbling and falling on the silo cover or the slippery silo floor. * Danger from falling silage masses at the removal point. * Falling from the cutting edge or the silo wall. x | | | F:\svlfg\400_Praevention\401_GuQ\02_Allgemein\70_Medien\15_Symbole\ASR A1.3\Warnzeichen\GIF\w008.gif |  |
|  | **PROTECTIVE MEASURES AND RULES OF CONDUCT** | | | | |  |
|  | F:\svlfg\400_Praevention\401_GuQ\02_Allgemein\70_Medien\15_Symbole\ASR A1.3\Gebotszeichen\m008.gif  F:\svlfg\400_Praevention\401_GuQ\02_Allgemein\70_Medien\15_Symbole\ASR A1.3\Gebotszeichen\m018.gif | x   * Prevent unauthorised individuals (onlookers) from entering the silo. * Employees and other involved parties (e.g. service providers) should receive instruction. * Wear safety shoes/boots (S3/S5). * Clean ascents of vehicles for silage or substrate removal regularly! * Do not jump on to or down from vehicles, e.g. for silage or substrate removal. Climb off backwards * Only use appropriate removal technology with a driver protection roof. * Avoid undercuts at the removal location or eliminate them immediately. * When uncovering the silo foil, a minimum distance of 2 metres from the cutting edge must be maintained. If necessary, suitable aids should be used to retract the film or remove the sandbags/tyres, or mobile railings or rope protection with suitable attachment points are used. * Mobile silo walls are secured against persons falling inwards and outwards, e.g. by railings or an embankment (vertical distance between the embankment and top edge of the wall 1 m). * Check protective devices for stability and functionality. x | | | F:\svlfg\400_Praevention\401_GuQ\02_Allgemein\70_Medien\15_Symbole\ASR A1.3\Verbotszeichen\GIF\d-p006.gif |  |
|  | **WHAT TO DO IN THE CASE OF MALFUNCTIONS** | | | | |  |
|  |  | * Immediately cordon off the danger areas! | | |  |  |
|  | **WHAT TO DO IN THE CASE OF ACCIDENTS – FIRST-AID – EMERGENCY TEL. NO. 112** | | | | |  |
|  | E004 Notruftelefon | * Carry out emergency measures at the scene of the accident! * Call the emergency services/an emergency doctor!   First aider:………………………………………………………………………………………... | | | E003 Erste Hilfe |  |
|  | **Maintenance** | | | | |  |
|  |  | * Replace or repair missing or damaged fall protection devices immediately! | | |  |  |
|  | **CONSEQUENCES OF NON-COMPLIANCE** | | | | |  |
|  |  | * Health consequences: Possibility of very serious or fatal injuries! x | | | www.svlfg.de |  |
|  |  | | | | |  |