|  |  |  |
| --- | --- | --- |
|   |        |   |
|  | **Company:** | **Operating Instructions** | **Date:** |   |
|   |   |
|   |   |
|   | **Working area:****stable complex** | **Activity: Working in the freestall barn** | **Signature:** |   |
|   |   |
|   |   |
|   | **DESIGNATION** |   |
|   | **Working in the freestall barn** |   |
|   |   |
|   |   |
|   | **DANGERS TO HUMANS AND THE ENVIRNOMENT** |   |
|   | W001 Allgemeines Warnzeichen (Dieses Zeichen darf nur in Verbindung mit einem Zusatzzeichen angewendet werden, das die Gefahr konkretisiert) | * Danger of slipping due to damp and smooth floors
* Being kicked or pushed by the cows
* Danger from electrical installations.
* Danger from dust, liquid manure gases and animal hair allergens
* Risksm from zoonoses
 | W011 Warnung vor Rutschgefahr |   |
|   | **PROTECTIVE MEASURES AND RULES OF CONDUCT** |   |
|   | F:\svlfg\400_Praevention\401_GuQ\02_Allgemein\70_Medien\15_Symbole\ASR A1.3\Gebotszeichen\m008.gif  F:\svlfg\400_Praevention\401_GuQ\02_Allgemein\70_Medien\15_Symbole\ASR A1.3\Gebotszeichen\m010.gif | * Use anti-slip floor coverings and keep them clean.
* Wear safety shoes/boots (S3/S5).
* Deploy only instructed and trained individuals to deal with cattle.
* Provide immobilisation devices such as a grab feeding fence or treatment stand.
* Immobilise cattle in immobilisation devices during treatments or examinations.
* Stud bulls are to be kept in a separate stud bull box if possible.
* Stable complexes with free-running stud bulls are not to be entered without assistants.
* Create a personnel pass-through as an escape route from the animal area.
* Avoid dust formation and animal hair allergens in the stable (e.g. bind meal-containing feed with liquid, store concentrated feed in the outside silo, if possible attach a cow brush outside the stable).
* When stirring liquid manure, open all stable gates and windows wide!
* Immediately treat cattle with infectious diseases (e.g. calf lichen).
* In stables with slide-type manure removal systems, the run-up points on winches and deflection rollers must be effectively secured against access.
* Fans suspended deeper than 2.70 m must be secured against access with a protective grille.
* Have the electrical system checked regularly by a specialist. Check the function of the residual current circuit breaker (30 mA) (press the test button). Applies to the entire socket circuits.
* Electrically operated roller shutters and curtains must be equipped with an automatic switch-off device or a dead man's switch.

  | F:\svlfg\400_Praevention\401_GuQ\02_Allgemein\70_Medien\15_Symbole\ASR A1.3\Gebotszeichen\m009.gif |   |
|   | **WHAT TO DO IN THE CASE OF MALFUNCTIONS** |   |
|   |  | * Repair defective structural equipment or report a requirement.
* Report any cattle with behavioural problems and remove them from the herd.
* In the event of malfunctions in the electrical system, contact a specialist company.
 |  |   |
|   | **WHAT TO DO IN THE CASE OF ACCIDENTS – FIRST-AID – EMERGENCY TEL. NO. 112** |   |
|   | E004 Notruftelefon | * Carry out emergency measures at the scene of the accident!
* Call the emergency services/an emergency doctor!

 First aider:…………………………………………………………………………………... | E003 Erste Hilfe |   |
|   | **MAINTENANCE** |   |
|   |  | * Check the systems and equipment before starting work.
* Observe the manufacturer's specifications for maintenance intervals.
 |  |   |
|  | **CONSEQUENCES OF NON-COMPLIANCE** |  |
|  |  | * Health consequences: injury, illness!
 | www.svlfg.de |  |
|   |       |  |