|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  | | | | |  |
|  | **Company:** | | **Operating Instructions** | **Date:** | |  |
|  |  |
|  |  |
|  | **Working area:**  **stable complex** | | **Activity: Working in the freestall barn** | **Signature:** | |  |
|  |  |
|  |  |
|  | **DESIGNATION** | | | | |  |
|  | **Working in the freestall barn** | | | | |  |
|  |  |
|  |  |
|  | **DANGERS TO HUMANS AND THE ENVIRNOMENT** | | | | |  |
|  | W001 Allgemeines Warnzeichen (Dieses Zeichen darf nur in Verbindung mit einem Zusatzzeichen angewendet werden, das die Gefahr konkretisiert) | * Danger of slipping due to damp and smooth floors * Being kicked or pushed by the cows * Danger from electrical installations. * Danger from dust, liquid manure gases and animal hair allergens * Risksm from zoonoses | | | W011 Warnung vor Rutschgefahr |  |
|  | **PROTECTIVE MEASURES AND RULES OF CONDUCT** | | | | |  |
|  | F:\svlfg\400_Praevention\401_GuQ\02_Allgemein\70_Medien\15_Symbole\ASR A1.3\Gebotszeichen\m008.gif    F:\svlfg\400_Praevention\401_GuQ\02_Allgemein\70_Medien\15_Symbole\ASR A1.3\Gebotszeichen\m010.gif | * Use anti-slip floor coverings and keep them clean. * Wear safety shoes/boots (S3/S5). * Deploy only instructed and trained individuals to deal with cattle. * Provide immobilisation devices such as a grab feeding fence or treatment stand. * Immobilise cattle in immobilisation devices during treatments or examinations. * Stud bulls are to be kept in a separate stud bull box if possible. * Stable complexes with free-running stud bulls are not to be entered without assistants. * Create a personnel pass-through as an escape route from the animal area. * Avoid dust formation and animal hair allergens in the stable (e.g. bind meal-containing feed with liquid, store concentrated feed in the outside silo, if possible attach a cow brush outside the stable). * When stirring liquid manure, open all stable gates and windows wide! * Immediately treat cattle with infectious diseases (e.g. calf lichen). * In stables with slide-type manure removal systems, the run-up points on winches and deflection rollers must be effectively secured against access. * Fans suspended deeper than 2.70 m must be secured against access with a protective grille. * Have the electrical system checked regularly by a specialist. Check the function of the residual current circuit breaker (30 mA) (press the test button). Applies to the entire socket circuits. * Electrically operated roller shutters and curtains must be equipped with an automatic switch-off device or a dead man's switch. | | | F:\svlfg\400_Praevention\401_GuQ\02_Allgemein\70_Medien\15_Symbole\ASR A1.3\Gebotszeichen\m009.gif |  |
|  | **WHAT TO DO IN THE CASE OF MALFUNCTIONS** | | | | |  |
|  |  | * Repair defective structural equipment or report a requirement. * Report any cattle with behavioural problems and remove them from the herd. * In the event of malfunctions in the electrical system, contact a specialist company. | | |  |  |
|  | **WHAT TO DO IN THE CASE OF ACCIDENTS – FIRST-AID – EMERGENCY TEL. NO. 112** | | | | |  |
|  | E004 Notruftelefon | * Carry out emergency measures at the scene of the accident! * Call the emergency services/an emergency doctor!   First aider:…………………………………………………………………………………... | | | E003 Erste Hilfe |  |
|  | **MAINTENANCE** | | | | |  |
|  |  | * Check the systems and equipment before starting work. * Observe the manufacturer's specifications for maintenance intervals. | | |  |  |
|  | **CONSEQUENCES OF NON-COMPLIANCE** | | | | |  |
|  |  | * Health consequences: injury, illness! | | | www.svlfg.de |  |
|  |  | | | | |  |