|  |  |  |
| --- | --- | --- |
|   |        |   |
|  | **Firm:** | **Operating Instructions** | **Date:** |   |
|   |   |
|   |  |   |
|   | **Work area:** | **Activity:** | **Signature:** |   |
|   |   |
|   |   |
|   | **DESIGNATION** |   |
|   | **Compact Loader** |   |
|   |   |
|   | **Loading and Transport Work** |   |
|   | **DANGERS TO PEOPLE AND THE ENVIRONMENT** |   |
|   |  | ▪ Danger of being run over▪ Danger due to slipping when getting on and off▪ Danger from turning over▪ Danger from hydraulic oil leaking under high pressure▪ Danger from falling objects (in particular large bales)▪ Danger from remaining in the danger area  |  |   |
|   | **PROTECTIVE MEASURES AND RULES OF CONDUCT** |   |
|   |  | **Foot protection:****Hearing protection:** | Wear safety shoes!Wear hearing protection at more than 80 dB(A)! |  |   |
| **Behaviour:**▪ Only to be operated by reliable individuals who have received instruction and been asked to operate the device by the company▪ The accident prevention regulations and the manufacturer‘s operating instructions must be complied with!▪ To be checked **before** use: Service and parking brake, working tools, steering, hydraulics,  lifting device, lighting and warning device.▪ **During** use: Check the condition and load-bearing capacity of the road surface – transport load in the lowest position, be aware of the increased risk of tilting with full steering lock and a raised load – therefore drive at an appropriate speed.▪ **Parking** the vehicle: Lower the lifting device, operate the parking brake, remove the key.▪ Do not remain in the danger area.▪ Riding on the machine or working equipment is prohibited!▪ Use a banksman if the visibility is not good.▪ For stacking and unstacking large bales use only vehicles with a cabin or protective roof for the driver. ▪ Move folding protective devices to the protective position.▪ Use the driver restraint system during all operations.▪ Don´t smoke when refuelling! |
|   | **WHAT TO DO IN THE CASE OF MALFUNCTIONS** |   |
|   |  | **Fire:****Malfunction:** | ▪ Fight incipient fires with a fire extinguisher – call the fire brigade!▪ In the case of danger, stop the engine immediately!▪ For maintenance, cleaning and repair work: Remove the ignition key and wait  until the engine has come to a standstill, then lower the load!▪ Continue working only after the malfunction has been repaired by trained personnel! |  |   |
|   | **WHAT TO DO IN THE CASE OF ACCIDENTS - FIRST AID - EMERGENCY CALL 112** |   |
|   |  | ▪ Carry out emergency measures at the scene of the accident!▪ Call an ambulance/doctor!▪ Inform superiors and professional association!First aider: ………………………………………………………………………………………….. |  |   |
|   | **MAINTENANCE** |   |
|   |  | ▪ Always check the function and safety equipment of the machine before switching on!▪ Comply with the manufacturer’s instuctions regarding care and maintenance!▪ Have repairs carried out only by trained personnel! |  |   |
|  | **CONSEQUENCES OF NON-COMPLIANCE** |  |
|  |  | ▪ Consequences for health: Injuries and illness!▪ Consequences under employment law: Warning, reprimand! |  |  |
|   |       |  |