|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  | | | | |  |
|  | **Firm:** | | **Operating Instructions** | **Date:** | |  |
|  |  |
|  |  |  |
|  | **Work area:** | | **Activity:** | **Signature:** | |  |
|  |  |
|  |  |
|  | **DESIGNATION** | | | | |  |
|  | **Compact Loader** | | | | |  |
|  |  |
|  | **Loading and Transport Work** | | | | |  |
|  | **DANGERS TO PEOPLE AND THE ENVIRONMENT** | | | | |  |
|  |  | ▪ Danger of being run over  ▪ Danger due to slipping when getting on and off  ▪ Danger from turning over  ▪ Danger from hydraulic oil leaking under high pressure  ▪ Danger from falling objects (in particular large bales)  ▪ Danger from remaining in the danger area | | |  |  |
|  | **PROTECTIVE MEASURES AND RULES OF CONDUCT** | | | | |  |
|  |  | **Foot protection:**  **Hearing protection:** | Wear safety shoes!  Wear hearing protection at more than 80 dB(A)! | |  |  |
| **Behaviour:**  ▪ Only to be operated by reliable individuals who have received instruction and been asked to operate  the device by the company  ▪ The accident prevention regulations and the manufacturer‘s operating instructions must be complied with!  ▪ To be checked **before** use: Service and parking brake, working tools, steering, hydraulics,  lifting device, lighting and warning device.  ▪ **During** use: Check the condition and load-bearing capacity of the road surface – transport load in the lowest  position, be aware of the increased risk of tilting with full steering lock and a raised load – therefore drive at  an appropriate speed.  ▪ **Parking** the vehicle: Lower the lifting device, operate the parking brake, remove the key.  ▪ Do not remain in the danger area.  ▪ Riding on the machine or working equipment is prohibited!  ▪ Use a banksman if the visibility is not good.  ▪ For stacking and unstacking large bales use only vehicles with a cabin or protective roof for the driver.  ▪ Move folding protective devices to the protective position.  ▪ Use the driver restraint system during all operations.  ▪ Don´t smoke when refuelling! | | |
|  | **WHAT TO DO IN THE CASE OF MALFUNCTIONS** | | | | |  |
|  |  | **Fire:**  **Malfunction:** | ▪ Fight incipient fires with a fire extinguisher – call the fire brigade!  ▪ In the case of danger, stop the engine immediately!  ▪ For maintenance, cleaning and repair work: Remove the ignition key and wait   until the engine has come to a standstill, then lower the load!  ▪ Continue working only after the malfunction has been repaired by trained personnel! | |  |  |
|  | **WHAT TO DO IN THE CASE OF ACCIDENTS - FIRST AID - EMERGENCY CALL 112** | | | | |  |
|  |  | ▪ Carry out emergency measures at the scene of the accident!  ▪ Call an ambulance/doctor!  ▪ Inform superiors and professional association!  First aider: ………………………………………………………………………………………….. | | |  |  |
|  | **MAINTENANCE** | | | | |  |
|  |  | ▪ Always check the function and safety equipment of the machine before switching on!  ▪ Comply with the manufacturer’s instuctions regarding care and maintenance!  ▪ Have repairs carried out only by trained personnel! | | |  |  |
|  | **CONSEQUENCES OF NON-COMPLIANCE** | | | | |  |
|  |  | ▪ Consequences for health: Injuries and illness!  ▪ Consequences under employment law: Warning, reprimand! | | |  |  |
|  |  | | | | |  |